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#322CN – Thermwood CNC Router CS45:
· Moving Gantry/Fixed Table - 60" width x 120" deep stationary aluminum table, the precision cast jig plate table top is equipped with integral spacers to allow for maximum vacuum flow. 

· Spindle - One (1) 10 HP, 3,000 to 24,000 RPM unit using ISO 30 tooling, programmable variable speed router spindle mounted to a servo controlled Z-axis

· Seven Position Bar Tool Holder for ISO 30 tooling

· Machine Frame - Engineered steel construction, the gantry construction consists of an engineered steel weldment of structural C chanel and steel plates

· Drive System - HIgh performance closed loop Siemens AC servos and ball screw drives on all axes, the ways on all axes are precision ground, hardened ways with precision bearings

· Rapid traverse - up to 1200 inches per minute

· Automatic Lubrication System – Automatically provides continuous lubrication to the rail bearings and the ball followers on the screws. Air requirements, 30 PSI, 5 CFM

· Vacuum - 18 HP Bekker vacuum pump

· Bar Code Reader System – Hand held reader allows user to read an existing bar code and automatically loads the correct corresponding part program to be executed

· Portable Hand Held Programming Unit – Equipped with keyboard and hand wheel/pulse generator. Provides full programming, lines, arcs, speed control, and editing. Programming features can be performed at the control system

· Control System - The 91000 SuperControl is feature rich, high performance CNC control system configured to perform 3 axis simultaneous motions. It is a multi-processor, full multi-tasking control. It features a high level of hardware integration, extensive use of reliable surface mount technology and a built in upgrade path for future technology. The control is equipped with a 14” full color monitor, 85 key 101 emulation QWERTY keyboard, 40 Gigabyte hard disk drive, 3 ½”, 1.4 Mb disk drive. It also includes a serial port for hand held programmer interface, variable 0 to 120% feed rate override and operator controls for start, stop, axis jog +, axis jog -, block step +, block step - and feed hold. The control provides AT bus expansion slots and is compatible with most Local Area Networks (LANs) as well as a variety of peripheral computer devices. The control uses a “Windows” operating system, offering the operator choices for program and machine operation display, pop up windows for event and information display, pop up windows for data input, and the ability to operate the machine in the background while doing other tasks on the control
Selling Price: $68,000.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY. SPECIFICATIONS ARE NOT ALWAYS EXACT AND ARE SUBJECT TO VERIFICATION. 
