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#317CN – Glue Line:
Glue line, consists of Comac glue spreader, Evans Machinery laminating index table, Evans Machinery pinch roller, Italpress 6 cylinder press. Comac Glue spreader: model C2R160, year of mfg 2000, twin rubber rollers, working width 1600mm, working thickness 100mm, feed speed 20 m/min, gear motor 0.5HP, 750 kg. weight. Evans index table, model 4253, provides for a single sheet of substrate to be laminated on both sides, conveys the board from the glue spreader and automatically positions and drops it on the bottom sheet of laminate with a minimal amount of effort by the operator, operator then places the top sheet on the board, 43" working height in-feed, foot print 177" x 87", maximum board size 61" x 145", working height out-feed 40".  

Selling Price: $38,000.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.
