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#224CN – Fezer JAT 28 Cross Feed Splicer:
Cross feed veneer splicer 2.8 meter capacity, year of mfg. 1993, 9.3 HP motor, veneer thickness 0.6 - 3.0 mm, min. veneer width 80mm, infeed speed adjustable from 0 to 45 m/min, outfeed speed adjustable from 0 to 60 m/min, slow speed adjustable from 0 to 15 m/min, width of heating plates 113 mm, total heated length 2.82 m, press beam stroke 20 - 120mm, working temperature adjustable from 100 to 200C, splicing pressure 5 - 16 bar, installed heating power 18 kW, heat up time 12 min, total installed power 23 kW, power demand 13.8 kW, net weight 4,840 kg, built-in hydraulic unit with air cooler to keep temp from rising above recommended limits, built-in clipper with hydraulic command, knife cutting against rotating roll, stainless steel heaters independently fed by electronic controller, auto sheet alignment.
Selling Price: $.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.
