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#198CN – Activa Edgebander:
Single sided edgebander, never used, year of mfg. 2008, capacity thickness of edgebanding 0.5 - 3mm, working thickness 11-40mm, minimum width 90mm, working length 280mm, 1st aggregate guillotine end trim, 2nd aggregate top and bottom trim, 2nd aggregate 370w, glue pot 1250w, glue pot maximum temp 200 degrees C, track motor 370w, edgeband drive motor 25w, glue pot drive motor 40w, configuration: hot melt glue, end trim, fine trim.
Selling Price: $12,600.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.
