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#343CN – Homag Edgebander:
Homag KL73/A3 edgebander with Doucet return conveyor, year 2002, 3mm PVC capability, top pressure with motorized height adjustment, HOMATIC control with input unit NC21, electronic frequency converters, hot melt glue system, feed infinitely variable 18 - 24m/min, working height 950mm, working width min. 55mm for panel thickness 22mm, min. 100mm for panel thickness 60mm, panel overhang 30mm, panel thickness 12 - 60mm, edge material on rolls 0.3 - 3mm, edge cross section max. with PVC 135mm2, with veneer 100mm2, roll diameter max. 830mm, pneumatic connection 7 - 8 bar, rough trim, fine trim, radius cutters, profile scraping unit, edge buffing top and bottom with oscillation.
Selling Price: $40,000.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY. SPECIFICATIONS ARE NOT ALWAYS EXACT AND ARE SUBJECT TO VERIFICATION. 
