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#344CN – Biesse Akron 425 Edgebander:
Biesse Edgebander, model Akron 425, year 2007, 6” colour touch screen controller, motorized pressure beam, VC-511 glue system, RPT pressure system, front and rear end trim w/tilt, top and bottom profile scraping unit, top and bottom edge scraping unit, top and bottom buffing unit, top and bottom hot air blower, min. panel thickness 10mm, max panel thickness 60mm, height of edge band material 14 – 64mm, min banding thickness 0.4mm, max. banding thickness 8mm, min. panel length 140mm, min. panel width 50mm, feed speed 13m/min, multi tap electrics.
Selling Price: $33,000.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY. SPECIFICATIONS ARE NOT ALWAYS EXACT AND ARE SUBJECT TO VERIFICATION. 
