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#282CN – Shaw Almex Membrane Press:
Model TL6-59-114, very good condition, year of mfg. 2006, single tray; 59" x 114" heated platen dimensions; 51" x 106" maximum usable area with 1.25" deep tray; working table height - 35"; maximum air bag pressure - 100 PSI; stroke of airbag - 1.75"; height of press chamber - 2.25"; Allen Bradley PLC control with Panelview 550 touchscreen; on board modem for diagnostics; 240 gallon storage pressure tank with check valve; 3 HP Busch vacuum pump with 240 gallon tank and valves; aluminum upper heating platen with nichrome heating element, insulation and digital temperature control; unheated solid aluminum lower platen; membrane clamp holds the membrane in place, it also introduces air pressure and vacuum into the pressing chamber beneath the membrane; (1) 14-roll vinyl rack 12' high, with cutter and ionization system to eliminate static electricity; pressing time depends on the type and thickness of the laminate, the press temperature, the adhesive formula and other factors; due to the number of variants it is impossible to accurately predict the press time, however a pressing cycle of 120 seconds can be achieved with most standard thermoplastic foils. Installed power supply: 60 amps on 480 volts; Necessary line air pressure - 120 PSI; Machine weight: 25,000 lbs.
Selling Price: $92,000US.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.
