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#216CN – Fisher & Ruckle Splicemaster:
Veneer splicer for pre glued veneer flitches, max. working width 47-1/2", veneer thickness .4 - 3mm, min. veneer length 11-4/5" to unlimited max. length, min. veneer width 1-3/4" - 47-1/4", variable feed speed 16 - 164 FPM, heating section length 47-1/4", max. heating temperature to approx. 220 degrees C.
Selling Price: $20,000.
USED MACHINERY IS SOLD ON AN “AS IS” BASES AND IS NOT COVERED UNDER WARRANTY.
